PORC327157-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

porc3271 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 87 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { porc3271 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        ErrorCrc Unsigned16,
    Chanel1 Unsigned16,
    Monitor Unsigned16,

}

ErrorCrc     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 Chanel1     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Monitor     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 

END

