POTM3205SFP49f-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

potm3205sfp4 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 159 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { potm3205sfp4 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        Input Unsigned16,
    GrSel Unsigned16,
    Ton Unsigned16,
    Gain12Db Unsigned16,
    Gain34Db Unsigned16,
    Strip Unsigned16,
    Vu Unsigned16,
    VuPos Unsigned16,
    VuScale Unsigned16,
    AudioDet Unsigned16,
    ErrEdhMin Unsigned16,
    ErrEdhHour Unsigned16,
    WavelengthNm Unsigned16,
    TxDbm Unsigned16,
    Rs232 Unsigned16,
    Rs422 Unsigned16,

}

Input     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Cs (0), 
    Cd (1), 
    Sd (2), 
    Br (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 GrSel     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 Ton     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    1 (2), 
    2 (3), 
    3 (4), 
    4 (5), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Gain12Db     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 Gain34Db     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 Strip     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    Auto (2), 
    1 (3), 
    2 (4), 
    3 (5), 
    4 (6), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 Vu     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 VuPos     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 VuScale     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Dbfs (0), 
    Dbu (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 AudioDet     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 ErrEdhMin     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 ErrEdhHour     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 WavelengthNm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 TxDbm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 Rs232     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 15 }
 Rs422     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 16 }
 

END

