PORC3225SFP4a0-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

porc3225sfp4 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 160 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { porc3225sfp4 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        GroupSelect Unsigned16,
    VideoStd Unsigned16,
    AssignA Unsigned16,
    TonA Unsigned16,
    GainA Unsigned16,
    AssignB Unsigned16,
    TonB Unsigned16,
    GainB Unsigned16,
    Vu Unsigned16,
    VuPos Unsigned16,
    VuScale Unsigned16,
    Vits Unsigned16,
    AudioDetect Unsigned16,
    EdhErrMin Unsigned16,
    EdhErrHour Unsigned16,
    RxDbm Unsigned16,
    Rs232 Unsigned16,
    Rs422 Unsigned16,

}

GroupSelect     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 VideoStd     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Cs (0), 
    Sdi (1), 
    Pal (2), 
    Secam (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 AssignA     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    12 (0), 
    21 (1), 
    11 (2), 
    22 (3), 
    34 (4), 
    43 (5), 
    33 (6), 
    44 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 TonA     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    L (2), 
    R (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 GainA     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 AssignB     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    12 (0), 
    21 (1), 
    11 (2), 
    22 (3), 
    34 (4), 
    43 (5), 
    33 (6), 
    44 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 TonB     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    L (2), 
    R (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 GainB     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 Vu     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 VuPos     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 VuScale     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Dbfs (0), 
    Dbu (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 Vits     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 AudioDetect     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 EdhErrMin     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 EdhErrHour     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 15 }
 RxDbm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 16 }
 Rs232     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 17 }
 Rs422     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 18 }
 

END

