PDVA7338bb-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

pdva7338 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 187 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { pdva7338 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        3G Unsigned16,
    Gr1 Unsigned16,
    Gr2 Unsigned16,
    Gr3 Unsigned16,
    Gr4 Unsigned16,
    Vu1 Unsigned16,
    Vu1Assign Unsigned16,
    Vu1Pos Unsigned16,
    Vu2 Unsigned16,
    Vu2Assign Unsigned16,
    Vu2Pos Unsigned16,
    Monitor Unsigned16,
    Reclocking Unsigned16,
    Detect Unsigned16,
    ErrHour Unsigned16,
    ErrMin Unsigned16,

}

3G     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Stream1 (0), 
    Stream2 (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 Gr1     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Gr2     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 Gr3     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 Gr4     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 Vu1     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 Vu1Assign     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Gr1 (0), 
    Gr2 (1), 
    Gr3 (2), 
    Gr4 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 Vu1Pos     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 Vu2     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 Vu2Assign     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Gr1 (0), 
    Gr2 (1), 
    Gr3 (2), 
    Gr4 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 Vu2Pos     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 Monitor     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Vu112 (0), 
    Vu134 (1), 
    Vu212 (2), 
    Vu234 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 Reclocking     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Dis (0), 
    En (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 Detect     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Edh (0), 
    Asi (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 15 }
 ErrHour     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 16 }
 ErrMin     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 17 }
 

END

