PFPC3353ae-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

pfpc3353 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 174 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { pfpc3353 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        T Unsigned16,
    TOc Unsigned16,
    5V Unsigned16,
    5V Unsigned16,
    V Unsigned16,
    V Unsigned16,
    V Unsigned16,
    V Unsigned16,
    Threshold Unsigned16,
    FansControl Unsigned16,
    FrameFan Unsigned16,
    FrameFanRpm Unsigned16,
    Pwr1Fan Unsigned16,
    Pwr1FanRpm Unsigned16,
    Pwr2Fan Unsigned16,
    Pwr2FanRpm Unsigned16,

}

T     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 TOc     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 5V     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 5V     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 V     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 V     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 V     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 V     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 Threshold     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 FansControl     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    All (1), 
    Pwr1 (2), 
    Pwr2 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 FrameFan     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 FrameFanRpm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 Pwr1Fan     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 Pwr1FanRpm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 Pwr2Fan     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 15 }
 Pwr2FanRpm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 16 }
 

END

