PEXT311876-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

pext3118 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 118 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { pext3118 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        SelGr Unsigned16,
    SelOut Unsigned16,
    OutAssign Unsigned16,
    Swap Unsigned16,
    6DbA Unsigned16,
    6DbB Unsigned16,
    TonA Unsigned16,
    TonB Unsigned16,
    AudioMon Unsigned16,
    MonPos Unsigned16,

}

SelGr     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 SelOut     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    A (0), 
    B (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 OutAssign     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Swap     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 6DbA     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 6DbB     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 TonA     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    Left (2), 
    Right (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 TonB     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    Left (2), 
    Right (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 AudioMon     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 MonPos     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 

END

