PDDA31063XB74-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

pdda31063xb MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 116 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { pdda31063xb 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        AudGainDb Unsigned16,
    MonVolDb Unsigned16,
    Test Unsigned16,
    Freq Unsigned16,
    Unlock Unsigned16,
    Conf Unsigned16,
    Bip Unsigned16,
    Par Unsigned16,
    Valid Unsigned16,
    Aud Unsigned16,

}

AudGainDb     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 MonVolDb     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 Test     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    Lm (2), 
    Mr (3), 
    Mm (4), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Freq     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 Unlock     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 Conf     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 Bip     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 Par     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 Valid     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 Aud     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 

END

