PORC3234SFP4b2-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

porc3234sfp4 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 178 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { porc3234sfp4 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        Gr Unsigned16,
    AssignA Unsigned16,
    TonA Unsigned16,
    GainADb Unsigned16,
    AssignB Unsigned16,
    TonB Unsigned16,
    GainBDb Unsigned16,
    VuScale Unsigned16,
    Aud Unsigned16,
    EdhM Unsigned16,
    EdhH Unsigned16,
    RxDbm Unsigned16,
    Rs232 Unsigned16,
    Rs422 Unsigned16,

}

Gr     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 AssignA     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    12 (0), 
    21 (1), 
    11 (2), 
    22 (3), 
    34 (4), 
    43 (5), 
    33 (6), 
    44 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 TonA     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    L (2), 
    R (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 GainADb     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 AssignB     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    12 (0), 
    21 (1), 
    11 (2), 
    22 (3), 
    34 (4), 
    43 (5), 
    33 (6), 
    44 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 TonB     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Lr (1), 
    L (2), 
    R (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 GainBDb     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 VuScale     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Dbfs (0), 
    Dbu (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 Aud     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 EdhM     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 EdhH     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 RxDbm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 Rs232     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 Rs422     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 

END

