PSSY3082SP38-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

pssy3082sp MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 56 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { pssy3082sp 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        LockH Unsigned16,
    LockCol Unsigned16,
    HTim Unsigned16,
    VTim Unsigned16,
    Agc Unsigned16,
    Scl1 Unsigned16,
    Scl2 Unsigned16,
    Freeze Unsigned16,
    TestH Unsigned16,
    Vblk Unsigned16,

}

LockH     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 LockCol     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 HTim     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 VTim     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 Agc     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 Scl1     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 Scl2     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 Freeze     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 TestH     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 Vblk     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 

END

