PENC30056-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

penc3005 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 6 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { penc3005 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        Test Unsigned16,
    Std Unsigned16,
    Vbi Unsigned16,
    Vits Unsigned16,
    RefEn Unsigned16,
    PalLock Unsigned16,
    PalSc Unsigned16,

}

Test     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    Bars (1), 
    1 (2), 
    2 (3), 
    3 (4), 
    4 (5), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 Std     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Pal (0), 
    Sec (1), 
    Yc (2), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 Vbi     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Blank (0), 
    Inp (1), 
    Ref (2), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Vits     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 RefEn     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 PalLock     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Sc (0), 
    Frm (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 PalSc     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 

END

