PORC7228486-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

porc72284 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 134 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { porc72284 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        InpMode Unsigned16,
    InpStd Unsigned16,
    Bars Unsigned16,
    AudioDet1 Unsigned16,
    AudioDet2 Unsigned16,
    AudioDet3 Unsigned16,
    AudioDet4 Unsigned16,
    VTim Unsigned16,
    HTim Unsigned16,
    OutGroup Unsigned16,
    Assign12 Unsigned16,
    InpSdi Unsigned16,
    ChMap Unsigned16,
    Assign34 Unsigned16,
    InpSdi Unsigned16,
    ChMap Unsigned16,
    Gain12Db Unsigned16,
    Gain34Db Unsigned16,
    Ton Unsigned16,
    VuMetr Unsigned16,
    VuPosition Unsigned16,
    RxDbm Unsigned16,
    EdhErrMin Unsigned16,
    EdhErrHour Unsigned16,
    ErrorReset Unsigned16,

}

InpMode     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Auto (0), 
    Manual (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 InpStd     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Sdi (0), 
    Hd1080 (1), 
    Hd720 (2), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 Bars     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 AudioDet1     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 AudioDet2     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 AudioDet3     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 AudioDet4     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 VTim     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 HTim     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 OutGroup     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    1 (0), 
    2 (1), 
    3 (2), 
    4 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 Assign12     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 InpSdi     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Gr1 (0), 
    Gr2 (1), 
    Gr3 (2), 
    Gr4 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 ChMap     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    12 (0), 
    21 (1), 
    11 (2), 
    22 (3), 
    34 (4), 
    43 (5), 
    33 (6), 
    44 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 Assign34     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 InpSdi     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Gr1 (0), 
    Gr2 (1), 
    Gr3 (2), 
    Gr4 (3), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 15 }
 ChMap     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    34 (0), 
    43 (1), 
    33 (2), 
    44 (3), 
    12 (4), 
    21 (5), 
    11 (6), 
    22 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 16 }
 Gain12Db     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 17 }
 Gain34Db     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 18 }
 Ton     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    1 (2), 
    2 (3), 
    12 (4), 
    3 (5), 
    4 (6), 
    34 (7), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 19 }
 VuMetr     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 20 }
 VuPosition     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 21 }
 RxDbm     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 22 }
 EdhErrMin     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 23 }
 EdhErrHour     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 24 }
 ErrorReset     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 25 }
 

END

