PTC205537-MIB DEFINITIONS ::= BEGIN

IMPORTS
  proflexCard FROM PROFLEX-CARD-MIB

  MODULE-IDENTITY FROM SNMPv2-SMI;

ptc2055 MODULE-IDENTITY
	LAST-UPDATED "201110050000Z"
	ORGANIZATION "www.profitt.ru"
	CONTACT-INFO
    "email:    info@profitt.ru"
  	DESCRIPTION
    "Top-level infrastructure of the proflex MIB tree"
    ::= { proflexCard 55 }

statusTable     OBJECT-TYPE
    SYNTAX      SEQUENCE OF proflexCardEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    ::= { ptc2055 1 }

statusTableEntry     OBJECT-TYPE
    SYNTAX      statusTableEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    INDEX       { proflexSlot }
    ::= { statusTable 1 }

statusTableEntry ::= SEQUENCE {
        Inp Unsigned16,
    Test Unsigned16,
    Afc Unsigned16,
    Vits Unsigned16,
    Ref Unsigned16,
    Out Unsigned16,
    Vbi Unsigned16,
    Black Unsigned16,
    Gain Unsigned16,
    Chr Unsigned16,
    Shrp Unsigned16,
    Sc Unsigned16,
    Ych Unsigned16,
    Ycv Unsigned16,
    Htim Unsigned16,
    Vtim Unsigned16,
    Frz Unsigned16,

}

Inp     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    1 (0), 
    2 (1), 
    Yc (2), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 1 }
 Test     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 2 }
 Afc     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Au (0), 
    Sl (1), 
    Fs (2), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 3 }
 Vits     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 4 }
 Ref     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 5 }
 Out     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    P (0), 
    S (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 6 }
 Vbi     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 7 }
 Black     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 8 }
 Gain     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 9 }
 Chr     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 10 }
 Shrp     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 11 }
 Sc     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 12 }
 Ych     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 13 }
 Ycv     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 14 }
 Htim     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 15 }
 Vtim     OBJECT-TYPE
    SYNTAX      Unsigned16
    
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 16 }
 Frz     OBJECT-TYPE
    SYNTAX      Unsigned16
    {
    Off (0), 
    On (1), 
    }
    MAX-ACCESS  read-only
    STATUS      current
    ::= { statusTableEntry 17 }
 

END

